{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["2mapping"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"2mapping","index":0,"n_rows":189,"n_cols":5,"rows_kept":189,"cut":false,"hidden":false,"merged":[]}
["1Spatial Rules","Description","Dimension_LD","Dimension","Category"]
["ALL-I-001","EnglishName metadata must be set if EnglishName is not empty","RepresentationalConciseness","LogicalConsistency","Representational"]
["ALL-I-002","EnglishName metadata must not be set if EnglishName is empty","RepresentationalConciseness","LogicalConsistency","Representational"]
["ALL-I-003","IrishName metadata must be set if IrishName is not empty","RepresentationalConciseness","LogicalConsistency","Representational"]
["ALL-I-004","IrishName metadata must not be set if IrishName is empty","RepresentationalConciseness","LogicalConsistency","Representational"]
["ALL-I-007","FunctionValue metadata must not be null","Consistency","LogicalConsistency","Intrinsic"]
["ART-I-006","Artificial polygons must be at least 1 sq m in area","Consistency","LogicalConsistency","Intrinsic"]
["ART-I-209","Artificial polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["ART-I-211","Artificial polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["ART-X-100","Artificial 'Built Environment' must have Building or Structure","Completeness","Completeness","Intrinsic"]
["BLD-I-003","Building Form Function combination must be correct","PositionalValidity","LogicalConsistency","Geospatial"]
["BLD-I-008","Building must have a Point geometry","Completeness","Completeness","Intrinsic"]
["BLD-I-009","Building pntGeomValue must be contained within the polygon of the Building","Completeness","Completeness","Intrinsic"]
["BLD-I-020","Building englishName must be at least 4 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-021","Building englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-022","Building englishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-023","Building irishName must be at least 4 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-024","Building irishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-025","Building irishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-026","Building bldNoValue must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-027","Building bldNoValue must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLD-I-031","Building must not have the same GeoId as another Building","SemanticAccuracy","ThematicAccuracy","Intrinsic"]
["BLD-I-209","Building polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["BLD-I-211","Building polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["BLD-X-100","Building must equal Artificial 'Built Environment' that it covers","Consistency","LogicalConsistency","Intrinsic"]
["BLD-X-101","Building polygons must not overlap","Consistency","LogicalConsistency","Intrinsic"]
["BLD-X-102","Building must not intersect Divisions other than InnerWall and OpenWall","Consistency","LogicalConsistency","Intrinsic"]
["BLDG-X-010","BuildingGroup must be referenced by at least 2 Buildings","Completeness","Completeness","Intrinsic"]
["BLDG-X-011","BuildingGroup geometry must be equal to the union of all Buildings that reference it","Consistency","LogicalConsistency","Intrinsic"]
["BLDU-I-026","BuildingUnit addrUnitNumber must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BLDU-X-101","BuildingUnit point must be contained within a Building polygon","Consistency","LogicalConsistency","Intrinsic"]
["BLP-I-006","BLP polygons must be at least 10 sq m in area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BLP-I-209","BLP polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["BLP-I-211","BLP polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["BLP-X-105","BLPs must not overlap","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BLP-X-106","BLP must not overlap a Way feature with funcValue 'Main Road', 'First Class', 'Second Class', 'Third Class', 'Fourth Class' or 'Fifth Class' and zOrder=0","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BLP-X-107","BLP must not overlap a Water feature with formValue 'River', 'Stream', 'Lake', 'Sea', 'Stream' or 'Canal' and zOrder=0","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BYA-I-018","BoundaryArea LEA englishName must contain valid formatting","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYA-I-019","BoundaryArea englishName must be set, for all types other than 'Baronial Water'","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYA-I-021","BoundaryArea englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYA-I-023","BoundaryArea irishName must be at least 3 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYA-I-024","BoundaryArea irishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYA-I-210","BoundaryArea of certain types must have a BdyId and EnglishName","RepresentationalConciseness","LogicalConsistency","Representational"]
["BYL-X-101","BoundaryLine of the same type cannot overlap","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BYL-X-102","BoundaryLine HWM must touch at least one other HWM BoundaryLine at its start","Completeness","Completeness","Intrinsic"]
["BYL-X-103","BoundaryLine HWM must touch at least one other HWM BoundaryLine at its end","Completeness","Completeness","Intrinsic"]
["BYL-X-104","BoundaryLine LWM must touch exactly one other LWM BoundaryLine at its start","Completeness","Completeness","Intrinsic"]
["BYL-X-105","BoundaryLine LWM must touch exactly one other LWM BoundaryLine at its end","Completeness","Completeness","Intrinsic"]
["BYM-I-205","BoundaryMereing must pass the OGC_simple test","SyntacticValidity","LogicalConsistency","Intrinsic"]
["BYM-I-206","BoundaryMereing must be at least 0.2m in length","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BYM-I-212","BoundaryMereing lines must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["BYM-X-101","BoundaryMereing cannot overlap","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BYM-X-103","BoundaryMereing must be contained within the outline of a BoundaryArea of a certain type","Completeness","Completeness","Intrinsic"]
["BYP-X-110","BoundaryPoints must not be within 1m of each other","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["BYP-X-111","BoundaryPoint must be on a BoundaryMereing","Completeness","Completeness","Intrinsic"]
["DIV-I-006","Division lines must be at least 0.1m in length","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["DIV-I-210","Division lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["DIV-I-212","Division lines must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["DIV-X-100","Division Open Wall must be contained within the boundary of exactly one Building","Consistency","LogicalConsistency","Intrinsic"]
["DIV-X-101","Division other than InnerWall or OpenWall can only touch Building","Consistency","LogicalConsistency","Intrinsic"]
["DIV-X-102","Division Inner Wall must be contained within 1 Building, or on the boundary between 2","Consistency","LogicalConsistency","Intrinsic"]
["DIV-X-103","Divisions at same ZOrder must be split where they intersect","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["DIV-X-104","Division must not intersect another Division at a 2 node","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["DIV-X-105","Division lines must not overlap","Consistency","LogicalConsistency","Intrinsic"]
["DIV-X-106","Division line Virtual Junction must be equal to the intersection of two Ways with the same Form Function","Consistency","LogicalConsistency","Intrinsic"]
["EXP-I-006","Exposed polygons must be at least 1 sq m in area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["EXP-I-209","Exposed polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["EXP-I-211","Exposed polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["EXP-X-125","Exposed 'Rock Face' must have Structure 'Top of Rock Face' on part of its boundary","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["LOC-I-003","Locale Form Function combination must be correct","PositionalValidity","LogicalConsistency","Geospatial"]
["LOC-I-006","Locale polygons must be at least 1 sq m in area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["LOC-I-020","Locale englishName must be at least 4 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["LOC-I-021","Locale englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["LOC-I-022","Locale englishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["LOC-I-023","Locale irishName must be at least 3 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["LOC-I-025","Locale irishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["LOC-I-209","Locale polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["RNS-I-006","RailNetworkSegment lines must be at least 0.5m in length","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["RNS-I-206","RailNetworkSegment lines must pass the OGC_simple test","PositionalValidity","LogicalConsistency","Geospatial"]
["RNS-I-210","RailNetworkSegment lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["RNS-I-212","RailNetworkSegment lines must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["RNS-X-100a","RailNetworkSegment must connect to a RailPoint at its Start","Completeness","Completeness","Intrinsic"]
["RNS-X-100b","RailNetworkSegment must connect to a RailPoint at its End","Completeness","Completeness","Intrinsic"]
["RNS-X-104a","RailNetworkSegment Start must not intersect another RailNetworkSegment at a 2 node","Consistency","LogicalConsistency","Intrinsic"]
["RNS-X-104b","RailNetworkSegment End must not intersect another RailNetworkSegment at a 2 node","Consistency","LogicalConsistency","Intrinsic"]
["RP-X-110","RailPoints must not be within 1m of each other","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["RP-X-130","RailPoint must connect to at least 1 RailNetworkSegment","Completeness","Completeness","Intrinsic"]
["RP-X-135","RailPoint Rail Switch must touch at least 3 RailNetworkSegment GDF1 lines","Completeness","Completeness","Intrinsic"]
["RP-X-136a","RailPoint 'End of Rail' must connect to exactly 1 GDF1 RailNetworkSegment","Completeness","Completeness","Intrinsic"]
["SL-I-210","ServiceLine lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["SOE-X-001","SoE must have no gaps or overlaps","Consistency","LogicalConsistency","Intrinsic"]
["ST-I-003","Site Form Function combination must be correct","Consistency","LogicalConsistency","Intrinsic"]
["ST-I-020","Site englishName must be at least 4 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["ST-I-021","Site englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["ST-I-022","Site englishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["ST-I-024","Site irishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["ST-I-209","Site polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["ST-I-211","Site polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["STP-X-002","Site point must be contained within the Site it references","Completeness","Completeness","Intrinsic"]
["STR-I-003","Structure Form Function combination must be correct","SemanticAccuracy","ThematicAccuracy","Intrinsic"]
["STR-I-004","Structure Function must not be 'Not Defined'","Completeness","Completeness","Intrinsic"]
["STR-I-020","Structure englishName must be at least 4 characters long","RepresentationalConciseness","LogicalConsistency","Representational"]
["STR-I-021","Structure englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["STR-I-022","Structure englishName must not start or end with a space","RepresentationalConciseness","LogicalConsistency","Representational"]
["STR-I-024","Structure irishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["STR-I-201","Structure polygons and closed lines must have at least 3 vertices","Completeness","Completeness","Intrinsic"]
["STR-I-205","Structure geometries must pass the OGC_simple test","PositionalValidity","LogicalConsistency","Geospatial"]
["STR-I-209","Structure geometries must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["STR-I-211","Structure geometries must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-101","Structure must not overlap other Structures of the same Form and Function","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-102","Structure 'Bridge Fixed' 'Multiple Use' must intersect some SoE at zOrder less than 0","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-110","Structure Points must not be within 0.4m of each other","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["STR-X-120","Structure 'Sluice Gate' must be contained within Water polygon","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-121","Structure with this Form must intersect a Water polygon","Completeness","Completeness","Intrinsic"]
["STR-X-122","Structure 'Landform' must have 'Landform Line' around its edge","Completeness","Completeness","Intrinsic"]
["STR-X-123","Structure 'Landform Line' must be contained within a 'Landform' polygon","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-124","Structure 'Top of Rock Face' must be ring oriented along the boundary of an Exposed 'Rock Face' polygon","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["STR-X-125","Structure 'Canopy' 'Building Overhang' must not overlap Built Environment","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-126","Structure 'Archway' must not overlap Built Environment","Consistency","LogicalConsistency","Intrinsic"]
["STR-X-127","Structure 'Archway' must overlap Buildings","Completeness","Completeness","Intrinsic"]
["STR-X-128","Structure 'Canopy' 'Building Overhang' must overlap Buildings","Completeness","Completeness","Intrinsic"]
["STR-X-131","Structure of this form must have Built Environment","Completeness","Completeness","Intrinsic"]
["STR-X-132","Structure Steps must be equal to 8th Class Way and Form must be equal to Walk General","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["STR-X-133","Structure Rail Platform must be equal to Artificial with functionValue Concrete Gravel Tarred Artificial Area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["VEG-I-006","Vegetation polygons must be at least 1 sq m in area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["VEG-I-209","Vegetation polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["VEG-I-211","Vegetation polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["WSS-I-006","WaterSingleStream lines must be at least 0.5m in length","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WSS-I-206","WaterSingleStream lines must pass the OGC_simple test","PositionalValidity","LogicalConsistency","Geospatial"]
["WSS-I-210","WaterSingleStream lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WSS-X-100a","WaterSingleStream must connect to a WaterPoint at its Start","Completeness","Completeness","Intrinsic"]
["WSS-X-100b","WaterSingleStream must connect to a WaterPoint at its End","Completeness","Completeness","Intrinsic"]
["WSS-X-104a","WaterSingleStream Start must not intersect another WaterSingleStream at a 2 node","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WSS-X-104b","WaterSingleStream End must not intersect another WaterSingleStream at a 2 node","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-I-006","Water polygons must be at least 1 sq m in area","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-I-007","Water lines must be at least 0.5m in length","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-I-008","Water must have lineGeomValue if Form in (River, Stream, Canal, Canal Lock, Mill Race)","Completeness","Completeness","Intrinsic"]
["WT-I-009","Water lineGeomValue must intersect its polygon boundary exactly twice","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-I-015b","Water salinityValue must be 'Saltwater' for this Form","SemanticAccuracy","ThematicAccuracy","Intrinsic"]
["WT-I-206","Water lines must pass the OGC_simple test","PositionalValidity","LogicalConsistency","Geospatial"]
["WT-I-209","Water polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WT-I-210","Water lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WT-I-211","Water polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["WT-X-100a","Water with lineGeomValue must connect to WaterPoint at its Start","Completeness","Completeness","Intrinsic"]
["WT-X-100b","Water with lineGeomValue must connect a WaterPoint at its End","Completeness","Completeness","Intrinsic"]
["WT-X-104a","Water lineGeomValue Start must not intersect another Water lineGeomValue at a 2 node","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-X-104b","Water lineGeomValue End must not intersect another Water lineGeomValue at a 2 node","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WT-X-105a","Water Start must follow same direction as connected Water","Completeness","Completeness","Intrinsic"]
["WT-X-105b","Water End must follow same direction as connected Water","Completeness","Completeness","Intrinsic"]
["WTP-X-100","WaterPoint must connect to at least 1 Water or WaterSingleStream except if 'Spring'","Completeness","Completeness","Intrinsic"]
["WTP-X-101","WaterPoint 'Issue Point' must connect to the Start of exactly 1 Water or WaterSingleStream","Consistency","LogicalConsistency","Intrinsic"]
["WTP-X-102","WaterPoint 'Sink Point' must connect to the End of exactly 1 Water or WaterSingleStream","Consistency","LogicalConsistency","Intrinsic"]
["WTP-X-110","WaterPoints must not be within 1m of each other","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WY-I-003","Way Form Function combination must be correct","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-006","Way polygons must be at least 1 sq m in area","SemanticAccuracy","ThematicAccuracy","Intrinsic"]
["WY-I-008","Way must have lineGeomValue if specific Form and Functions","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-009","Way lineGeomValue must intersect its polygon boundary exactly twice","Completeness","Completeness","Intrinsic"]
["WY-I-010","Way GDF2 reference must be set if specific Forms","Completeness","Completeness","Intrinsic"]
["WY-I-011","Way GDF2 reference must NOT be set if specific Forms","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-015a","Way accessModeValue must be 'Free' for this Form and Function combination","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-015c","Way accessModeValue must be 'Free' 'Toll' or 'Public Service Vehicle Only' for this Form and Function combination","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-015c","Way accessModeValue must be 'Free' or 'Toll' for this Form and Function combination","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-015e","Way accessModeValue must be 'Restricted' for this Form and Function combination","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-015f","Way accessModeValue must be 'Impossible' for this Form and Function combination","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-209","Way polygons must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-210","Way lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-211","Way polygons must not have Spikes","Consistency","LogicalConsistency","Intrinsic"]
["WY-I-220","Way with certain form and functions must have directionValue 'As Digitised'","Completeness","Completeness","Intrinsic"]
["WY-X-100a","Way with lineGeomValue must connect to a WayPoint at its Start","Completeness","Completeness","Intrinsic"]
["WY-X-100b","Way with lineGeomValue must connect to a WayPoint at its End","Completeness","Completeness","Intrinsic"]
["WY-X-101","Way Roundabout lines must be have clockwise direction and a directionValue 'As Digitised'","Completeness","Completeness","Intrinsic"]
["WY-X-104a","Way lineGeomValue Start must not intersect another Way lineGeomValue at a 2 node - exception for 'Virtual Junction' and 'Gate'","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WY-X-104b","Way lineGeomValue End must not intersect another Way lineGeomValue at a 2 node - exception for 'Virtual Junction' and 'Gate'","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WY-X-105","Way lineGeomValue must be contained within the WayGDF2 line it references","Completeness","Completeness","Intrinsic"]
["WY-X-107","Way must reference WayGDF2 with the same zOrderValue","Completeness","Completeness","Intrinsic"]
["WY-X-108","Way must reference WayGDF2 with the same Form and Function","Completeness","Completeness","Intrinsic"]
["WY-X-109","Way must reference WayGDF2 with the same Access Mode","Completeness","Completeness","Intrinsic"]
["WYG2-I-003","WayGDF2 Form Function combination must be correct","PositionalValidity","LogicalConsistency","Geospatial"]
["WYG2-I-206","WayGDF2 lines must pass the OGC_simple test","PositionalValidity","LogicalConsistency","Geospatial"]
["WYG2-I-210","WayGDF2 lines must not have Kickbacks","Consistency","LogicalConsistency","Intrinsic"]
["WYG2-X-100a","WayGDF2 must connect to a WayPoint at its Start","Completeness","Completeness","Intrinsic"]
["WYG2-X-103","WayGDF2 must be referenced by 1 to 5 Way features","Completeness","Completeness","Intrinsic"]
["WYG2-X-104a","WayGDF2 Start must not intersect another WayGDF2 at a 2 node - exception for 'Virtual Junction' and 'Gate'","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WYG2-X-104b","WayGDF2 End must not intersect another WayGDF2 at a 2 node - exception for 'Virtual Junction' and 'Gate'","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WYG2-X-107","WayGDF2 must be referenced by Way with the same zOrderValue","Completeness","Completeness","Intrinsic"]
["WYG2-X-108","WayGDF2 must be referenced by Way with the same Form and Function","Completeness","Completeness","Intrinsic"]
["WYP-I-021","WayPoint englishName must contain valid characters only","RepresentationalConciseness","LogicalConsistency","Representational"]
["WYP-X-110","WayPoints must not be within 1m of each other","PositionalAccuracy","PositionalAccuracy","Geospatial"]
["WYP-X-131","WayPoint must connect to at least 1 Way or WayGDF2","Completeness","Completeness","Intrinsic"]